ITEM #: ICE MACHINE  
Quantity: Two (2)  
Manufacturer: Scotsman  
Model No.: C1030MW-32A  
Pertinent Data: 1300 Pounds ARI Capacity, Water Cooled  
Utilities Req’d: 208230V/1PH, 14.8A; 3/8” CW, 3/4” IW, 3/8” Chilled Water Supply, 1/2” Chilled Water Return

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #, Water Filtration System.  
4. Install ice maker on top of Item #, Ice Bin, coordinate proper installation.  
5. Ice maker shall produce regular cubes 7/8” by 7/8” by 7/8” thick.  
6. Provide unit with VariSmart Ice Level Control.  
7. Provide ice machine with all necessary accessories to fit onto Item #, Ice Bin flawlessly.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.