ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Scotsman   
Model No.: C1848MR-32   
Pertinent Data: 1826 Pounds Capacity, Remote Cooled  
Utilities Req’d: 208-230V/1PH, 24.8A; 3/8" CW, 3/4" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
4. Install ice maker on top of Item #\_\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Ice maker shall produce regular cubes 7/8" by 7/8" by 7/8" thick.  
6. Provide unit with Vari-Smart Ice Level Control.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_\_, Ice Bin flawlessly.  
8. Coordinate installation with Item #\_\_\_\_\_,Compressor Rack for remote condensing unit.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.