ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: C1848SW-32  
Pertinent Data: 1900 Pounds Capacity, Water Cooled  
Utilities Req’d: 208-230V/1PH, 23.8A; 3/8" CW, 3/4" IW, 3/8" Chilled Water Supply,

1/2" Chilled Water Return  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
4. Install ice maker on top of Item #\_\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Ice maker shall produce small cubes 7/8" by 7/8" by 3/8" thick.  
6. Provide unit with KPAS which includes KVS Vari-Smart Ice Level Control, and KSBU-N Smart-Board Advance Control with Network.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_\_, Ice Bin, flawlessly.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.