ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: F0522W-1  
Pertinent Data: 429 Pounds ARI Capacity, Water Cooled  
Utilities Req’d: 120V/1PH, 14.4A; 3/8" CW, 3/4" IW, 3/8" Chilled Water Supply,

1/2" Chilled Water Return  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
4. Install ice maker on top of Item #\_\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Provide unit with KPAS which includes KVS Vari-Smart Ice Level Control, and KSBU-N Smart Board Advanced Control with Network.  
6. Ice maker shall produce flaked ice.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_\_, Ice Bin over 1/3 portion flawlessly.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.