ITEM #: ICE MAKER WITH BIN  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: CU1526SA-1  
Pertinent Data: 101 Pounds ARI Capacity, Air Cooled  
Utilities Req’d: 120V/1PH, 15.0A; 3/8" CW, 3/4" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
4. Install ice maker under Item #\_\_\_\_\_\_\_\_,\_\_\_\_\_\_\_\_, coordinate proper installation.  
5. Ice maker shall produce small cubes 7/8" by 7/8" by 3/8" thick.  
6. Provide unit with KPUFM26 Prodigy under counter floor mount.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.