ITEM #: ICE MAKER  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: IM-500SAB  
Pertinent Data: 414 Pounds ARI Capacity, Air Cooled  
Utilities Req’d: 120V/1PH, 11.5A; 1/2" CW, 3/4" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_, Water Filtration System.  
4. Install ice maker on top of Item #\_\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Provide unit with KPAS which includes KVS Vari-Smart Ice Level Control, and KSBU-N Smart Board Advanced Control with Network.  
6. Ice maker shall produce square cubes 1" by 1" by 1-1/4" thick.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_\_, Ice Bin, flawlessly.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.