ITEM #: IN COUNTER ESPRESSO MACHINE  
Quantity: One (1)  
Manufacturer: Modbar  
Model No.: AV1T  
Pertinent Data: 1 Group Tap System  
Utilities Req’d: 208V/1PH; 14.2A; 3/4” CW, 3/4” IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall be equipped with multi-position lever with four saved programs.  
4. Equip unit with pid temperature control.  
5. Provide the unit with simple heads-up display.  
6. Equip the unit with a heads-up shot timer.  
7. Unit shall have La Marzocco portafilters.  
8. Water Quality for this unit must meet Total Dissolved Solids 150 ppm, Total Hardness gpg, Total Alkalinity 80 ppm, pH 7.0 gpg, Calciu Hardness 3-4 gpg, Total Chlorine < 0.1 ppm, Free Chlorine <0.5, Total Chlorides< 30 ppm, Total Iron 0 mg/L, Silica 5mg/L, Sulfate 25-50 mg/L, Hydrogen Sulfide 0mg/L, Manganese 0mg/L, Nitrate 0mg/L.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.