ITEM #: INDUCTION BASE CHARGER  
Quantity: One (1)  
Manufacturer: Dinex  
Model No.: DXSMA2081  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH; 16.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide Smart·Therm induction charger constructed with the main body of stainless steel and composite induction friendly materials.  
4. Equip with a microprocessor that performs unique, patented and patent pending temperature control, automatic standby/shut-off and self-diagnostics.  
5. Provide user-friendly control buttons for ease of use and automatic power control.  
6. Provide visible LCD display and audible alert for precise user feedback.  
7. Unit to have automatic sensor for Dinex induction bases.  
8. Coordinate installation into the recess in Item #\_\_\_\_.