ITEM #: INDUCTION CHARGER  
Quantity: One (1)  
Manufacturer: Dinex  
Model No.: DX2011208  
Pertinent Data: ---  
Utilities Req’d: 208V/3PH; 20.0A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall be constructed with the main body of stainless steel and a heavy-duty composite surface.  
4. Equip with a microprocessor that performs unique, automatic standby/shut-off functions, self-diagnostics and incorporates a proprietary automatic sensor for use with Dinex® Induction Bases.  
5. Provide user-friendly control buttons for ease of use and automatic power control.  
6. Provide visible LCD display & audible alert for precise user feedback.  
7. Equip unit with a washable filter.  
8. Coordinate installation into the recess in Item #, Chef’s Counter with Sink and Plate Storage.   
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.