9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.  
  
ITEM #: INDUCTION COOKING STATION   
Quantity: One (1)  
Manufacturer: Spring USA  
Model No.: ICS348-18  
Pertinent Data: Mobile  
Utilities Req'd: 120V/1PH; 50.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide three (3) flush mounted MAX Induction Ranges, with 5mm thick, tempered glass cook tops.  
4. Provide individual SmartScan controls providing: voltage, pan size and pan type recognition, choice of power or temperature mode, ferrous pan recognition, and large LED power/temp display.  
5. Provide two (2) quiet downdraft AF-350 Air Filter Systems with stainless steel, counter-level, capture flue (s) washable pre-filter, primary cell filter & carbon absorption filter delivering 96.7% capture of 1-3 micron particulate.  
6. Coordinate installation of unit into Item #, Work Counter with Hand Sink Below.