7. Provide four (4) heavy duty, non-marking casters, two (2) with brakes.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.  
  
  
ITEM #: INDUCTION WARMER  
Quantity: One (1)  
Manufacturer: Cook Tek  
Model No.: B651-U2 (660801)  
Pertinent Data: Under Counter-Top Incogneto  
Utilities Req’d: 120V/1PH; 6.0A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit is to be placed on underside of Interior Designer supplied Counter-Top. Coordinate installation with General Contractor.  
4. See Plans Drawing Detail C FSD.106.  
5. Provide fixed position track system to mount unit to underside of counter-top.  
6. Provide unit with Cook Tek Magneeto 2 trivet.  
7. Provide unit with control panel and automatic pan detection.  
8. Standard induction compatible serving dishes are required for operation of unit.  
9. Unit shall be built with an auto shut-off feature to prevent overheating, offer self-diagnostics, and have a pan maximizer feature to ensure maximum heating of any induction compatible pan.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.