ITEM #: INDUCTION WARMER  
Quantity: One (1)  
Manufacturer: CookTek  
Model No.: MC1500 (600501)  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH; 14.0A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall be portable design with stainless steel housing.  
4. Equip unit with high temperature glass ceramic top.  
5. Provide high quality internal electronics and heavy-gauge Litz wire.  
6. Provide individual controls for each burner (hob).  
7. Equip unit with LED display.  
8. Equip unit with automatic pan detection.  
9. Unit shall be programmed with 22 temperature settings and 20 power cook settings.  
10. Provide unit with automatic shutoff feature prohibits overheating.  
11. Unit shall be equipped with a microprocessor which monitors vital components to check for overheating, and power supply issues.  
12. Provide 1.8 meter power cord coordinate NEMA configuration with Electrical Contractor.  
13. Coordinate installation onto Item #N724, Pastry Preparation Counter.  
14. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.