ITEM # : JUICE DISPENSER   
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: JDF-4S (37300.0000)  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 6.0A; 3/8” CW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Equip unit with a patented high density mixing system.  
3. Unit shall include both push and hold dispense and optional single size portion control.  
4. Provide unit with quick dispense with 1.0 to 1.5oz (29.6 to 44.4ml) per second flow rate  
5. Unit shall have the ability to delivers both frozen and ambient concentrate products.   
6. Equip the unit with a door lock.  
7. Provide unit with 7" cup clearance accommodates most juice containers  
8. Must meet all applicable governmental, and local laws, rules, regulations, and codes.