ITEM #: JUICE EXTRACTOR  
Quantity: One (1)  
Manufacturer: Zumex  
Model No.: Essential Pro   
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 2.7A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Verify with the Architect and or Interior Designer the desired color of the unit.  
4. Equip the unit with an integrated peel bucket.  
5. Unit shall be equipped with an Intuitive “Touch Control” digital display.  
6. Provide the unit with a total and partial fruit counter.  
7. Coordinate installation onto Item #, Butler Counter With Sink.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.