ITEM #: KEG BEER REFRIGERATOR  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: DDS60  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH; 5.5A; 3/4” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Keg Cooler shall be self-contained refrigeration with the condensing unit on the left.  
3. Unit shall be provided with heavy-duty cord and plug, coordinate NEMA configuration with electrical contractor.  
4. Provide stainless steel doors hinged left, right.  
5. Unit shall be built into a seamless top to give the appearance of a single work station.  
6. Coordinate installation of a single Beer Dispensing Tower with 2 faucets and a drip trough.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.