ITEM #: MEAL DELIVERY CART  
Quantity: One (1)  
Manufacturer: FWE  
Model No.: PTS3030  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 10.8A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with a built-in heat system to prevent tampering, loss or damage.  
4. Unit shall be provided with tamper proof controls.  
5. Provide a stainless steel rack assembly which can be customized to accommodate a wide variety of tray sizes.  
6. Provide 12-gauge, stainless steel hinges keep doors properly aligned for years of use, secured with tamperproof screws.  
7. Unit shall be fully heliarc welded construction with extra welds at critical points provides structural integrity to withstand rough handling no rivets.  
8. Provide a tamper resistant super duty full perimeter bumper.  
9. Provide tamper proof screws.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.