ITEM #308: MOBILE PLATE AND DISH DISPENSER  
Quantity: One (1)  
Manufacturer: Dinex  
Model No.: DXIDPH2E/1012  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 7.5A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide lifting mechanisms which shall be constructed of type 304 stainless steel with all exposed parts having a No. 4 finish.  
4. Provide two plate guides of high impact molded plastic which shall be securely mounted to the top flange.  
5. Provide a full complement of stainless steel extension springs shall be furnished which can be easily disconnected to adjust the lifting rate.  
6. Provide a floating plate suspended from the extension springs to support the stack of plates to be dispensed.  
7. Provide a stainless steel exterior shield furnished on each dispenser.  
8. Provide a heater and thermostat mounted in the base of the dispenser.  
9. Provide a lighted on/off switch which shall be mounted in one of the plastic plate guides on top of the dispenser.  
10. Provide four 5" casters, two (2) with brakes, and perimeter bumper.  
11. Provide heavy duty cord and plug, coordinate NEMA configuration with Electrical Contractor.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.