ITEM #: MOBILE REFRIGERATOR CABINET  
Quantity: One (1)  
Manufacturer: Carter Hoffman  
Model No.: PHB495HE  
Pertinent Data: Mobile  
Utilities Req’d: 120V/1PH; 7.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide self-contained evaporator coil and blower refrigeration system.  
3. Provide unit with flush mounted dial type thermometer, Lexan thermometer cover, with remote sensing bulb.   
4. Provide unit with top mounted transport latch.   
5. Provide unit with 6” swivel casters, two (2) with brakes.   
6. Provide unit with heavy duty cord and plug, coordinate NEMA configurations with electrical contractor.   
7. Provide removable extruded aluminum racks with extruded aluminum channel slides. Slides shall be fixed at 1-1/2” centers; accommodate 18” x 26” sheet pans.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.