ITEM #: MODULAR FOUR BURNER RANGE  
Quantity: One (1)  
Manufacturer: Imperial  
Model No.: IHR-4-M   
Pertinent Data: ---  
Utilities Req’d: 3/4” Gas @ 160,000 BTU’s; 5” WC

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide wavy grates.  
4. Provide 3/4” rear gas connection.  
5. Provide 3/4” gas shut off valve.  
6. Coordinate installation onto Item #, Refrigerated Equipment Stand.  
7. Provide cast iron design features flame shaping center tube for more efficient heat transfer.  
8. Provide 48” flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.