ITEM #: MODULAR HOT TOP RANGE  
Quantity: One (1)  
Manufacturer: Imperial  
Model No.: HR2HTM   
Pertinent Data: ---  
Utilities Req’d: 3/4” Gas @ 80,000 BTU’s; 5” WC  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide heavy-duty, highly polished plates.  
4. Provide burners which are located every 457 mm. Each burner has one manual control.  
5. Provide “U” shaped burners which have aeration baffles between burners for quick recovery.  
6. Provide 3/4” rear gas connection.  
7. Provide 3/4” gas shut off valve.  
8. Coordinate installation onto Item #, Refrigerated Equipment Stand.  
9. Provide 48” flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.