ITEM #: MODULAR HOT TOP RANGE  
Quantity: One (1)  
Manufacturer: Jade Range  
Model No.: JMRH-2HT  
Pertinent Data: ---  
Utilities Req’d: 3/4” Gas @ 70,000 BTU’s, 5” WC

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide 3/4” rear gas connection, cap and cover front gas manifold on both left and right side.  
4. Provide highly polished reinforced cast iron plates.  
5. Equip with one 35,000 BTU/hr burner per section.  
6. Provide 14-gauge all welded body construction.  
7. Unit shall have stainless steel gas tubing throughout.  
8. Equip unit with stainless steel front, sides and stub back.  
9. Provide unit with a stainless steel 6" plate shelf.  
10. Coordinate installation onto Item # ???  
11. Provide 48” flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.