ITEM #: MODULAR SIX BURNER RANGE  
Quantity: One (1)  
Manufacturer: Imperial  
Model No.: IHR6M  
Pertinent Data: ---  
Utilities Req’d: 3/4” Gas @ 210,000 BTUs; 5” WC  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide wavy grates.  
4. Provide anticlogging shield designed into the grate protects the pilot from grease and debris.  
5. Provide cast iron design features flame shaping center tube for more efficient heat transfer.  
6. Coordinate installation onto Item #, Refrigerated Equipment Stand.  
7. Equip unit with a LP Gas shutoff valve.  
8. Provide 48” flex, quick disconnect gas hose with restraining device and LP Gas pressure regulator.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.