ITEM #: MODULAR SIX BURNER RANGE  
Quantity: One (1)  
Manufacturer: Jade  
Model No.: JMRH4  
Pertinent Data: ---  
Utilities Req’d: 3/4” Gas @ 210,000 BTU’s, 5” WC

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide 3/4” rear gas connection, cap and cover front gas manifold on both left and right side.  
4. Unit shall be equipped with Individual lift off steel top grates.  
5. Equip unit with one stainless steel pilot per burner.  
6. Provide 14-gauge all welded body construction.  
7. Unit shall be equipped with stainless steel gas tubing throughout.  
8. Equip unit with Stainless steel front, sides, tray bed and stub back.  
9. Equip unit with 6” plate shelf.  
10. Coordinate installation onto Item #, Refrigerated Equipment Stand.  
11. Provide 48” flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.