ITEM #: MOP SINK CABINET  
Quantity: One (1)  
Manufacturer: Advance Tabco  
Model No.: 9-OPC-84DL-300  
Pertinent Data: ---  
Utilities Req’d: 1/2” CW, 1/2” HW, 2” DW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide heavy-gauge type 300 stainless steel construction.  
4. Provide a double door unit. Verify which side the mop sink is to be placed.  
5. Provide 16” x 20” x 12” deep heavy-gauge type 304 stainless steel mop sink.  
6. Provide a K240 service faucet, spray hose, and spray hose bracket.  
7. Provide louvers along the top of each side panel for ventilation.  
8. Provide a sloped top for ease of cleaning.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.