ITEM #: OIL CONTAINMENT CADDY  
Quantity: One (1)  
Manufacturer: Frontline  
Model No.: 10SS-NA-LP  
Pertinent Data: 10-Gallon Capacity  
Utilities Req’d: 120V/1PH; 3.5A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide heavy-gauge stainless-steel construction.  
4. Provide smooth, rolling, heavy-duty, non-mark casters, swivel front casters with brakes.  
5. Provide extra-large “crumb catcher” basket.  
6. Provide power switch and “break away” power cord.  
7. Provide removable handle and lock-in-place safety cover  
8. Provide high-temperature hose.  
9. Provide special filter screen to protect pump.  
10. Unit shall be UL, UL Sanitation Listed.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.