ITEM #: PANINI GRILL  
Quantity: One (1)  
Manufacturer: Electrolux  
Model No.: 602113  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH; 16.6A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall be made of stainless steel AISI 430 and the cooking surface is made of a special cast iron treated with verified food enamel, this guarantees hygienic conditions and high resistance to acids, salts and oxidation processes.  
4. Equip the unit with an adjustable thermostat up to 572°F (300˚C).  
5. Provide a self-balancing upper plate adjusts to different heights to reduce cooking times and double performance.  
6. Unit shall be equipped with shockproof heating elements mounted inside the plate for a perfect thermal conductivity.  
7. Provide a top plate on/off switch.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.