ITEM #: PASS THRU BAR REFRIGERATOR  
Quantity: One (1)  
Manufacturer: True Food Service Equipment   
Model No.: TBR60-PTSZ1-L-S-GG-GG-1  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH; 3.2A; 1" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide stainless steel interior.  
4. Provide exterior sides, top, and grill to be stainless steel, back and bottom to be galvanized steel.  
5. Provide four (4) glass doors with stainless steel frame.  
6. Provide unit with 7/8" roller castors.  
7. Coordinate installation under Item #  
8. Provide 3/4" diameter NSF brass drain.  
9. Provide 1/4 HP condensing unit as shown on drawings.  
10. Unit shall be provided with heavy duty cord and plug, coordinate NEMA configuration with electrical contractor.   
11. All refrigeration components are to meet NSF-7 requirements.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.