ITEM #: PASS-THRU REFRIGERATOR  
Quantity: One (1)  
Manufacturer: True Food Service Equipment   
Model No.: STR-1RPT-1S-1S-HC  
Pertinent Data: Single Section, Self-Contained  
Utilities Req’d: 120V/1PH; 3.8A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide stainless steel door, front and sides on the exterior, and stainless steel sides, wall and back on the interior.  
3. Provide four (4) 6” heavy-duty swivel casters two (2) with brakes.  
4. Provide heavy-duty cord and plug.  
5. Provide two (2) full-height solid doors, hinged as shown on plans.  
6. Provide two (2) additional wire shelves.  
7. KEC shall provide trim strips between the wall opening and the Refrigerators.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.