ITEM #: PASTA COOKER  
Quantity: One (1)  
Manufacturer: Jade Range  
Model No.: JTPC-18  
Pertinent Data: ---  
Utilities Req’d: 3/4” CW; 1” Gas @ 80,000 BTU’s, 5” WC; 1” IW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide an 11-gallon capacity removable tank.  
3. Provide a 12-gauge 316 stainless steel removable water tank.  
4. Provide a stainless steel cabinet interior and exterior.  
5. Provide piezo igniter, and automatic pilot.  
6. Unit shall be equipped with seamless stainless steel baskets with perforated holes.  
7. Provide infinite control manual gas valve.  
8. Provide top mount water dispenser.  
9. Provide 48” flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
10. Provide four (4) heavy-duty, non-marking casters, two (2) with brakes.  
11. Provide PosiSet.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.