ITEM #: PIZZA OVEN  
Quantity: One (1)  
Manufacturer: Wood Stone  
Model No.: WS-MS-6-RFG-IR  
Pertinent Data: Radiant Flame Gas Fired  
Utilities Req’d: 120V/1PH, 1.1A; 3/4” Gas @ 188,000 BTU’s  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place as shown on drawings.  
2. Provide with all standard accessories.  
3. Provide with mantle extension with black granite mantle.  
4. Provide stainless steel oven tool set.  
5. Provide extended storage box under granite mantle. extended storage box to be provided with a ventilation and access to the oven.  
6. Provide stainless steel trim strips at exposed areas between pizza oven and walls.  
7. Provide an easily adjustable 105,000 BTU wall of radiant flame located at the rear of the cooking chamber.  
8. Provide ceramic log set.  
9. KEC to coordinate all exterior finishes and needed trim with Interior Designer.  
10. Provide gas pressure regulator.  
11. Coordinate with Item #, Exhaust Hood.  
12. Provide shop drawings for approval prior to fabrication.  
13. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.