ITEM #: PLANCHA  
Quantity: One (1)  
Manufacturer: Jade  
Model No.: JTRH-36IP-36  
Pertinent Data: ---  
Utilities Req’d: 3/4” Gas @ 70,000 BTU’s; 5” WC  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with a polished 5/8” thick plancha plate.  
4. Unit shall be equipped with 14-gauge stainless steel grease trough.  
5. Provide stainless steel front sides and stub back.  
6. Equip unit with 6” plate shelf.  
7. Provide four (4) 6” high adjustable heavy-duty, non-marking casters, two (2) with brakes.  
8. Provide 14-gauge stainless steel interior sides rear and deck on oven.  
9. Provide 48” flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
10. Provide PosiSet.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.