ITEM #: PLASTIC DOOR  
Quantity: One (1)  
Manufacturer: Curtron  
Model No.: PolarPro  
Pertinent Data: Swing Door In Jamb Mounting  
Utilities Req’d:

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be constructed of reinforced nylon.  
3. All mounting hardware shall be stainless steel.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.