ITEM #: PORTABLE BAR  
Quantity: Four (4)  
Manufacturer: FWE  
Model No.: BBC-6  
Pertinent Data: ---  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide welded steel top and bottom frame.  
4. Provide raised marine front edge to slow spills.  
5. Provide six (6) heavy duty, polyurethane tire casters.  
6. Provide six (6) circuit sealed in cold plate.  
7. Provide 60-pound ice capacity with stainless steel sliding cover.  
8. Provide laminate exterior. Verify with the Architect and or Interior Designer of the proper color.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.