ITEM #572: POT AND PAN WASHER  
Quantity: One (1)  
Manufacturer: Champion  
Model No.: PP-20  
Pertinent Data: Split Door Type  
Utilities Req’d: 208V/3PH; 88.0A; 3/4" HW, 1-1/4” IW (Wash Water); 1/2” CW (Drain Tempering)

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit to be front-loading, split door design.  
3. Equipment unit with booster heater to provide 180°F/190°F hot sanitizing rinse.  
4. Unit to have 20 pan capacity.  
5. Provide external wash down hose with spray nozzle.  
6. Provide one (1) stainless steel utensil rack with two (2) hold down lids, and two (2) stainless steel inserts for bun/sheet pans.  
7. Unit to have recirculating wash water and 27 second wash/rinse cycle.  
8. Provide with push button control and information center.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.