ITEM #: POT SINK  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS  
Utilities Req’d: 3/4” HW, 3/4” CW; 2” IW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X Detail #1B, #2C, #4A, #5A, #50, #51, and #56.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Provide flanged feet on front feet only to secure to floor.  
5. Provide three (3) 14 gauge stainless steel rotary waste lever angle brackets.  
6. From left to right provide three (3) 26” x 26” x 15” deep sinks with rotary waste and connected rear overflow.  
7. Provide two (2) Type 4B faucets. Mount to splash behind sink compartments.  
8. Coordinate installation of Item #, Pot Shelf.  
9. Provide 16 gauge stainless steel rails and cross rails.  
10. Provide space under right drainboard for Item #, Trash Receptacle.  
11. Provide cutout in right drainboard for Item #, Food Waste Collector.  
12. Provide a fully enclosed side splash on the left side of the unit.  
13. Provide 22gauge stainless steel wall flashing, as shown on drawings #FS.  
14. Fabricate and install per NSF Standard 2, complete drawings, schedules, elevations, and details.  
15. All finished edges shall be #7 mirrored polish finish.  
16. Provide shop drawings for approval prior to fabrication.  
17. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.