ITEM #: POWER WASH SINK  
Quantity: One (1)  
Manufacturer: Duke Mfg  
Model No.: X-STREAM K-5000  
Pertinent Data: By Owner  
Utilities Req’d: 208V/3PH; 20.0A; 3/4" HW, 3/4" CW; 2" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per plans, details, and the following:  
1. Size and configuration as shown on drawings.  
2. Set in place in location as shown on drawings.  
3. Provide flanged feet on front only.  
4. Provide stainless steel bracket for Sink Control.  
5. Provide 14-gauge stainless steel rotary waste lever brackets, one per sink.  
6. Coordinate installation with Item #, Pot Shelf.  
7. Provide cut-out and weld for Item #, Collector.  
8. Provide from left to right, three (3) sinks, two (2) 36" long x 28" wide x 14" deep, and one (1) 36" x 28" x 18" deep.  
9. Provide stainless steel bracket for Collector control.  
10. KEC to provide 22-gauge stainless steel flashing from top of splash to bottom of pot shelf.  
11. Provide minimum 12" back splash.  
12. Provide two (2) Type 4B faucets.  
13. Provide unit with raised roll end.  
14. Provide stainless steel legs and cross bracing.  
15. Provide unit with five variable speeds, and five timed programmable cycles.  
16. Provide unit with low water detection, change water indicator, and integrated soap dispensing.  
17. Provide unit with plug n’ play components, self-diagnostics, idle speed, data recording package, and integrated heated sanitizer.  
18. Provide 2500 Watt tank heater.  
19. Provide integrated pump drain valve, which opens when main wash engine is drained.  
20. Provide shop drawings for approval prior to fabrication.  
21. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.