ITEM #: POWER WASH SINK  
Quantity: One (1)  
Manufacturer: Powersoak  
Model No.: PS 6531  
Pertinent Data: Left to Right Operation See Drawing FS  
Utilities Req’d: 208V/3PH 26.7A; (2) 3/4" CW, (2) 3/4" HW, 2" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per plans, details, and the following:  
1. Size and configuration as shown on drawings.  
2. Set in place in location as shown on drawings.  
3. Provide flanged feet, anchored to floor, on front only.  
4. Provide stainless steel bracket for Sink Control.  
5. Provide 14-gauge stainless steel rotary waste lever brackets, one per sink.  
6. Coordinate installation with Item #51, Pot Shelf.  
7. Provide cut-out and weld for Item #53, Scrap Collector.  
8. Provide from left to left, three (3) sinks, one (1) 48" x 28" x 21" deep, and two (2) 24" long x 28" wide x 14" deep.  
9. Provide stainless steel bracket for Item #53, Scrap Collector Control Panel.  
10. KEC to provide 22-gauge stainless steel flashing from top of splash to bottom of pot shelf.  
11. Provide minimum 12" back splash.  
12. Provide two (2) Type 4B faucets.  
13. Provide stainless steel legs and cross bracing.  
14. Provide shop drawings for approval prior to fabrication.  
15. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.