ITEM #: PREPARATION COUNTER WITH SINK  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS  
Utilities Req'd: (2) 120V/1PH, 20.0A (Convenience Outlet); ½” CW, ½” HW, 1-1/2” IW

See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X Detail #1A, #2B, #4B, #5A, and #15.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Provide flanged feet, anchored to floor, on front legs only.  
5. Provide hinged cabinet doors with integrally formed full length door pull and intermediate shelves.  
6. Provide one (1) 14 gauge stainless steel rotary waste lever angle brackets.  
7. Provide one (1) 18” x 21” x 12” deep sink with rotary waste and connected rear overflow.  
8. Coordinate installation of Type 3C Faucet.  
9. Provide cutouts in counter top for Item #, Recessed Cutting Board, Item #, Trash Chute, and Item #, Under Counter Refrigerator with Drawers and Rail.  
10. Provide cutouts and space under counter for Item #, Under Counter Refrigerator with Drawers and Rail, and Item #, Trash Receptacle.  
11. Coordinate installation of Item # Double Wall Shelf.  
12. Fabricate and install per NSF Standard 2, complete drawings, schedules, elevations, and details.  
13. Provide shop drawings for approval prior to fabrication.  
14. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.