ITEM #: PULPER SYSTEM  
Quantity: One (1)  
Manufacturer: Somat  
Model No.: D-5 Disposer  
Pertinent Data: ---  
Utilities Req’d: 208V/3PH; 20.0A; 1/2" HW, 1/2" CW; 1-1/2" IW; 2" Slurry Inlet, 2" Slurry Outlet  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide 18" cone for installation into Item #, Pot Wash Sink.  
3. Provide NEMA 4 stainless steel Som-A-Trol recessed control center.  
4. KEC to coordinate with General Contractor and provide a fully operational and tested system.  
5. Provide unit with pulper pump to pump slurry to and from Item #, Pulper Extractor.  
6. Provide shop drawings for approval prior to installation.  
7. Provide with solenoid valve, syphon breaker, and flow control valve.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.