ITEM #: RAPID COOK OVEN  
Quantity: One (1)  
Manufacturer: Merry Chef  
Model No.: eikon e2s  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH, 20.0A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Coordinate installation on top of Item #, Freezer Worktop.  
4. Provide stainless steel finish.  
5. Provide a rail surrounding accessory storage on top of the oven.  
6. Equip unit with accelerated Cooking Technology7 which combines three heat technologies:  
a. Tuned impingement.  
b. Microwave.  
c. Convection.  
7. Provide ventless cooking capabilities through built-in catalytic converter.  
8. Provide a cool touch exterior.  
9. Provide EasyTouch7, icon driven touchscreen controls.  
10. Equip unit with USB memory stick data transfer of up to 1,024 cooking profiles.  
11. Unit shall be equipped with inbuilt diagnostic testing.  
12. Provide stainless steel cavity and case work.  
13. Provide a 12” cavity in a 14” width footprint.  
14. Provide the following accessories:  
a. Flat cook plate.  
b. Two cook plate liners.  
c. Solid base baskets: full, half and quarter sizes available in black and green.  
d. Guarded hand paddle with supporting side walls.  
e. Cool down pan.  
f. Merchandising panel.  
g. Merrychef cleaner.  
h. Merrychef protector.  
i. Other accessories by request.  
15. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.