ITEM #: RAPID COOK OVEN  
Quantity: One (1)  
Manufacturer: Turbo Chef  
Model No.: I3-9500-1  
Pertinent Data: Ventless  
Utilities Req’d: 208V/1PH; 40.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide countertop rapid cook oven with type 304 stainless steel interior and fully insulated cook chamber.  
4, Provide stainless steel front, top and sides.  
5. Provide 304 stainless steel removable grease collection pan and a removable rack.  
6. Equip with pull down door with ergonomic handle and side hand grips.  
7. Unit to have internal catalytic converter and smart voltage sensor technology.  
8. Provide digital display.  
9. Provide multi-speed impingement blower.  
10. Provide (2) solid PTFE baskets.  
11. Provide TurboChef Cleaner and Guard Starter Kit that includes (1) cleaner packet, (1) 24oz bottle, (1) Guard bottle and (2) foamer trigger, (1) standard rack.  
12. Provide 6’ cord and plug.  
13. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.