ITEM #: REACH-IN REFRIGERATED MERCHANDISER  
Quantity: One (1)  
Manufacturer: True Food Service Equipment   
Model No.: GDM-41SL-HC-LD  
Pertinent Data: Double Section  
Utilities Req’d: 120V/1PH, 10.8A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a sliding glass door merchandiser with two sliding doors of “Low-E”, double pane thermal insulated glass door assemblies with mitered plastic channel frames.   
4. Equip with self-closing doors. Counter-balanced weight system for smooth, even, positive closing.  
5. Provide eight (8) adjustable, heavy duty PVC coated wire shelves 20 7/8”L x 161/4”D (531 mm x 413 mm). Four (4) chrome plated shelf clips included per shelf.   
6. Equip with shelf support pilasters made of same material as cabinet interior; shelves are adjustable on 1/2” (13 mm) increments.  
7. Provide LED interior lighting provides more even lighting throughout the cabinet. Safety shielded.   
8. Exterior of cabinet shall be non-peel or chip black powder coated cold rolled steel; durable and permanent.   
9. Interior of cabinet shall be attractive, NSF approved, white aluminum liner with stainless steel floor.   
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.