ITEM #: REACH-IN REFRIGERATOR  
Quantity: One (1)  
Manufacturer: True Food Service Equipment  
Model No.: GDM-49-HC~TSL01  
Pertinent Data: Double Section, Self-Contained  
Utilities Req’d: 120V/1PH; 7.3A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide, non-peel or chip black powder coated cold rolled steel on the front and front and sides on the exterior, and aluminum liner with stainless steel floor on the interior.  
3. Provide four (4) 5” heavy-duty swivel casters two (2) with brakes.  
4. Provide heavy-duty cord and plug.  
5. Provide two (2) full-height double paned thermal insulated glass doors, hinged as shown on plans.  
6. Provide door locks.  
7. Provide two (2) additional shelves.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.