ITEM #: REACH-IN REFRIGERATOR  
Quantity: Two (2)  
Manufacturer: True  
Model No.: GDM-23-HST-HC  
Pertinent Data: Mobile, With Glass Door  
Utilities Req’d: 120V/1PH; 5.4A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide non-peel or chip black powder coated steel on the front and sides on the exterior, and white aluminum liner with stainless steel floor on the interior.  
3. Provide four (4) 6” heavy-duty swivel casters two (2) with brakes.  
4. Provide heavy-duty cord and plug.  
5. Provide Low-E thermal glass hinged door, hinged right side as shown on plans.  
6. Provide LED interior lights.  
7. Provide two (2) additional wire shelves.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.