ITEM #: RECESSED CUTTING BOARD  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Polymer  
Pertinent Data: See Plans Drawing #FS  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings  
2. Size and configuration as shown on drawings.  
2. Coordinate installation onto Item #, Garde Manger Counter With Sinks.  
3. Provide 1/2” thick removable Polyurethane cutting board.  
4. Recessed Cutting Board shall be removable/reversible and recessed into table and held in place by stainless steel pins and tabs.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.