ITEM #: REFRIGERATED BASE  
Quantity: One (1)  
Manufacturer: Jade Range  
Model No.: JRLH-04S-T-72  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH; 12.6A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Units construction shall be cabinet interiors, front, face and sides to be stainless steel.  
3. Equip drawer faces to have flush mount pull handle. Face and back to be stainless steel, and be self-closing drawers which have 14-gauge stainless steel drawer track, with 2" heavy-duty skate wheel.  
4. Provide heavy-duty rubber drawer gaskets.  
5. Provide with heavy-duty cord and plug. Coordinate NEMA configuration with Electrical Contractor.  
6. Equip with drawers which are to be easily removable for cleaning, and to accommodate 6" deep 12" x 20" hotel pans.  
7. Provide face mounted dial thermometers.  
8. Equip unit with a Condensing unit that uses R-404 refrigerant unless otherwise specified and a blower coil evaporator with R-404 expansion valve.  
9. Provide Six (6) 6” heavy-duty, non-marking casters, front two (2) with brakes.  
10. Coordinate installation of Item #???, ???? on top of unit.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.