ITEM #: REFRIGERATED COLD PAN  
Quantity: One (1)  
Manufacturer: Wells Mfg.  
Model No.: RCP-200  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH; 5.5A; 1” IW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide Stainless steel top and liner.  
4. Provide On/Off Switch with 8’ cord and plug.  
5. Provide recessed ledge for pan support and colder fresher products.  
6. Unit shall meet NSF Standard 2.  
7. Provide a five-year compressor warranty.  
8. Coordinate installation into Item #, Servery Counter with Tray Slide.  
9. Provide the following accessories:  
a. 5-year compressor warranty.  
b. Perforated bottom strainer plate.  
c. Adaptor bars for fractional sized pans.  
d. Remote on/off switch e. 220/230/240V.  
f. 50 cycle.  
g. Remote models (Includes compressor and condensing units and up to 20’ leads).  
h. Remote models without compressors or condensing units.  
i. Special condenser orientation and/or compressor rack position.  
j. 2nd year parts & labor warranty.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.