ITEM #: REFRIGERATED COLD WELL  
Quantity: One (1)  
Manufacturer: Wells Mfg.  
Model No.: RCP-400  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH, 5.5A, 1@ IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide factory installed drain, and valve.  
3. Provide self-contained unit.  
4. Provide recessed top edge.  
5. Provide unit with remote on/off switch.  
6. Provide the following accessories:  
a. 5-year compressor warranty.  
b. Perforated bottom strainer plate.  
c. Adaptor bars for fractional sized pans.  
d. Remote on/off switch e. 220/230/240V.  
f. 50 cycle.  
g. Remote models (Includes compressor and condensing units and up to 20’ leads).  
h. Remote models without compressors or condensing units.  
i. Special condenser orientation and/or compressor rack position.  
j. 2nd year parts & labor warranty.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.