ITEM #53: REVERSE OSMOSIS STORAGE TANK  
Quantity: One (1)  
Manufacturer: Pentair  
Model No.: ROMATE 60  
Pertinent Data: For Item #\_\_\_\_\_\_\_\_  
Utilities Req’d: 1-1/4" CW (From Item #\_\_\_\_\_)  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a 24” diameter 41.5” tall tank.  
4. Provide 60.0-gallon capacity with a 17.7 gallon draw down based on 60 psi.  
5. Coordinate installation with Item #\_\_\_\_, Reverse Osmosis System.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.