ITEM #: REVERSE OSMOSIS STORAGE TANK  
Quantity: One (1)  
Manufacturer: WaterSpec  
Model No.: ROST44  
Pertinent Data: For Item #  
Utilities Req’d: 3/8” CW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a 21” diameter 36.25” tall tank.  
4. Provide 44.0 gallon capacity with a 29 gallon draw down based on 60 psi.  
5. Coordinate installation with Item #, Reverse Osmosis System.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.